	Model Name	L4160 Series	
	Status	Fatal error	
	Firmware ver.	LW29JB 29/11/2019	
	MAC-ID String	F8:D0:27:4B:2E:EF	
	Serial Number	X4E5027545	
	Print Head ID	3A89C77R0L	
	First TI received time	04/06/2019	
	Manual cleaning counter	0	
	Timer cleaning counter	1	
	Ink replacement cleaning counter	0	
	Total print pass counter	421	
	Total print page counter - rear feed	14	
	Total scan counter	5	
	Ink replacement counter - black	0	
	Ink replacement counter - cyan	0	
	Ink replacement counter - magenta	0	
	Ink replacement counter - yellow	0	
	Last printer fatal error code 1	0x84D4 Paper jam error. Foreign object. Deformation. Change lever failure. Paper jam.	
	Last printer fatal error code 2	0x84D4 Paper jam error. Foreign object. Deformation. Change lever failure. Paper jam.	
	Last printer fatal error code 3	0x2B PF PID reverse error. Encoder failure. Tooth skip or improper tension of the timing belt. Paper jam. Motor driver failure. Main board failure.	
	Last printer fatal error code 4	0xEA61 Factor other than printer device error. Scanner or ADF failure.	
	Last printer fatal error code 5	0xEA61 Factor other than printer device error. Scanner or ADF failure.	
	Last scanner fatal error code 1	0x4D Scanner/ADF FB BS+ excess load error. Encoder failure. Tooth skip or improper tension of the timing belt. Gear crack. Cable or FFC disconnection. Motor driver failure. Main board failure.	
	Last scanner fatal error code 2	0x45 Scanner/ADF FB PID excess load error. Encoder failure. Tooth skip or improper tension of the timing belt. Gear crack. Cable or FFC disconnection. Motor driver failure. Main board failure.	
	Last scanner fatal error code 3	0x4D Scanner/ADF FB BS+ excess load error. Encoder failure. Tooth skip or improper tension of the timing belt. Gear crack. Cable or FFC disconnection. Motor driver failure. Main board failure.	
	Last scanner fatal error code 4	0x4D Scanner/ADF FB BS+ excess load error. Encoder failure. Tooth skip or improper tension of the timing belt. Gear crack. Cable or FFC disconnection. Motor driver failure. Main board failure.	
	Last scanner fatal error code 5	0x10 Scanner/ADF home position detection error. CIS Module failure. Upper housing failure. Lower housing failure. Scanner motor failure. Insufficient grease. Foreign object. Cable disconnection. Main board failure.	
	Last general fatal error code 1	0x13EE Board Failure (CARD).	
	Last general fatal error code 2	0x13EE Board Failure (CARD).	
	Last general fatal error code 3	0x13EE Board Failure (CARD).	
	Last general fatal error code 4	0x13EE Board Failure (CARD).	
	Last general fatal error code 5	0x13EE Board Failure (CARD).	
